Duct Test Report

|  |  |  |
| --- | --- | --- |
| **Testing Company** | **Name of Tester** | **Signature** |
| **A picture containing hanger  Description automatically generated** |  |  |
|  |  |  |
| **Home Address** | **Permit Number** | **GPIN** |
|  |  |  |
| **Conditioned Square footage** | **Source of Conditioned Square Footage** | **Number of HVAC Systems** |
|  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **TEST RESULTS** | | | |
| **System 1** |  |  |  |
| Duct tightness testing is not required. All ducts and the air handler are located entirely within the building thermal envelope. | | | |
| **Square Footage Served** | **Test Conditions** | **Maximum Allowed (CFM25)** | **Photo of Test Results on Gauge** |
|  |  |  |
| **Date** | **Test results (cfm@25pa)** | **Compliance Status** |
|  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **System 2** |  |  |  |
| Duct tightness testing is not required. All ducts and the air handler are located entirely within the building thermal envelope. | | | |
| **Square Footage Served** | **Test Conditions** | **Maximum Allowed (CFM25)** | **Photo of Test Results on Gauge** |
|  |  |  |
| **Date** | **Test results (cfm@25pa)** | **Compliance Status** |
|  |  |  |

**Notes**

**N1103.3.4 (R403.3.4) Duct Leakage (Prescriptive)**

|  |  |  |
| --- | --- | --- |
| **Test Conditions** | **Maximum Allowed Duct Leakage** | **Maximum Allowed (CFM25)** |
| Rough-in with air handler installed | 4 CFM per 100 sq ft of conditioned floor area | .04 x conditioned floor area served |
| Rough-in without air handler installed | 3 CFM per 100 sq ft of conditioned floor area | .03 x conditioned floor area served |
| Post-construction | 4 CFM per 100 sq ft of conditioned floor area | .03 x conditioned floor area served |

Logo

Description automatically generatedLogo, company name

Description automatically generatedLogo, company name

Description automatically generated